Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 638
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 632
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 463
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 1
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 3
Node:      0, Layer:    AppCbrServer, (0) Client address: 8
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.170485086
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.214520394
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.168154241
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      0, Layer:    AppCbrClient, (1) Server address: 8
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150202239046, end = 150545718597 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 184185 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 932
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 938
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 432
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 6
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150267146318, end = 150549147297 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 224339 bps
Node:      1, Layer:    AppCbrServer, (0) Client address: 7
Node:      1, Layer:    AppCbrServer, (0) First packet received at [s]: 0.221701270
Node:      1, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.245015752
Node:      1, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.180728956
Node:      1, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      1, Layer:    AppCbrClient, (0) Server address: 7
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1860
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 2760
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 541
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 2
Node:      2, Layer:    AppCbrServer, (0) Client address: 11
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.199719161
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.185307356
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.216977290
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      2, Layer:    AppCbrServer, (0) Client address: 14
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.163177433
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.088525191
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.169660133
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      2, Layer:    AppCbrServer, (0) Client address: 4
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.148573388
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.059288131
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.157228904
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      2, Layer:    AppCbrServer, (0) Client address: 6
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.133915290
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.170603696
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.163661663
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      2, Layer:    AppCbrClient, (1) Server address: 6
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150264101365, end = 160264101365 ns (closed), bytes sent = 28 B, bytes recv = 1130 B, throughput = 22 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1260
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 1560
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 480
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 84
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 8
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150265793665, end = 160277438830 ns (closed), bytes sent = 1130 B, bytes recv =  28 B, throughput = 22 bps
Node:      3, Layer:    AppCbrServer, (0) Client address: 15
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.141200181
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.118447272
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.161365422
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      3, Layer:    AppCbrServer, (0) Client address: 5
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.112057088
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.268328952
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.175832599
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      3, Layer:    AppCbrClient, (0) Server address: 5
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      4, Layer:          802.11, pkts from network: 0
Node:      4, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      4, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      4, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      4, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, retx pkts due to CTS timeout: 438
Node:      4, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      4, Layer:          802.11, pkt drops due to retx limit: 0
Node:      4, Layer:          802.11, RTS Packets ignored due to Busy Channel 60
Node:      4, Layer:          802.11, RTS Packets ignored due to NAV 8
Node:      4, Layer:    AppCbrClient, (0) Server address: 2
Node:      4, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      4, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      4, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      4, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      4, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      4, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      5, Layer:          802.11, pkts from network: 0
Node:      5, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:      5, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      5, Layer:          802.11, UCAST pkts rcvd clearly: 1200
Node:      5, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      5, Layer:          802.11, retx pkts due to CTS timeout: 471
Node:      5, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      5, Layer:          802.11, pkt drops due to retx limit: 0
Node:      5, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      5, Layer:          802.11, RTS Packets ignored due to NAV 2
Node:      5, Layer:    AppCbrServer, (0) Client address: 3
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.192318986
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.260684552
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.177636786
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      5, Layer:    AppCbrServer, (0) Client address: 13
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.185050982
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.163189676
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.169358562
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      5, Layer:    AppCbrClient, (0) Server address: 3
Node:      5, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      5, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      5, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      5, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      5, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      5, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      6, Layer:          802.11, pkts from network: 0
Node:      6, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:      6, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      6, Layer:          802.11, UCAST pkts rcvd clearly: 1200
Node:      6, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, retx pkts due to CTS timeout: 455
Node:      6, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      6, Layer:          802.11, pkt drops due to retx limit: 0
Node:      6, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      6, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      6, Layer:    AppCbrServer, (1) Client address: 2
Node:      6, Layer:    AppCbrServer, (1) First packet received at [s]: 0.214418797
Node:      6, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.237736310
Node:      6, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.163428727
Node:      6, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (1) Throughput (bits per second): 6002
Node:      6, Layer:    AppCbrServer, (0) Client address: 12
Node:      6, Layer:    AppCbrServer, (0) First packet received at [s]: 0.177772067
Node:      6, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.148466530
Node:      6, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.162800697
Node:      6, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      6, Layer:    AppCbrClient, (0) Server address: 2
Node:      6, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      6, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      6, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      6, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      6, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      6, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      7, Layer:          802.11, pkts from network: 0
Node:      7, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1200
Node:      7, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      7, Layer:          802.11, UCAST pkts rcvd clearly: 1500
Node:      7, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      7, Layer:          802.11, retx pkts due to CTS timeout: 487
Node:      7, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      7, Layer:          802.11, pkt drops due to retx limit: 0
Node:      7, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      7, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      7, Layer:    AppCbrServer, (0) Client address: 10
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.259280645
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.276133352
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.234153458
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      7, Layer:    AppCbrServer, (0) Client address: 1
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.155897566
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.252820152
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.181704182
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      7, Layer:    AppCbrClient, (0) Server address: 1
Node:      7, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      7, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      7, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      7, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      7, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      7, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      8, Layer:          802.11, pkts from network: 0
Node:      8, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      8, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      8, Layer:          802.11, UCAST pkts rcvd clearly: 900
Node:      8, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, retx pkts due to CTS timeout: 438
Node:      8, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      8, Layer:          802.11, pkt drops due to retx limit: 0
Node:      8, Layer:          802.11, RTS Packets ignored due to Busy Channel 59
Node:      8, Layer:          802.11, RTS Packets ignored due to NAV 9
Node:      8, Layer:    AppCbrServer, (0) Client address: 9
Node:      8, Layer:    AppCbrServer, (0) First packet received at [s]: 0.273858031
Node:      8, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.222084794
Node:      8, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.255180298
Node:      8, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      8, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      8, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      8, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      8, Layer:    AppCbrServer, (1) Client address: 0
Node:      8, Layer:    AppCbrServer, (1) First packet received at [s]: 0.251854829
Node:      8, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.177879056
Node:      8, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.172756727
Node:      8, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      8, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      8, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      8, Layer:    AppCbrServer, (1) Throughput (bits per second): 6002
Node:      8, Layer:    AppCbrClient, (0) Server address: 0
Node:      8, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      8, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      8, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      8, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      8, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      8, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      9, Layer:          802.11, pkts from network: 0
Node:      9, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      9, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      9, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:      9, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      9, Layer:          802.11, retx pkts due to CTS timeout: 438
Node:      9, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      9, Layer:          802.11, pkt drops due to retx limit: 0
Node:      9, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      9, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      9, Layer:    AppCbrClient, (0) Server address: 8
Node:      9, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      9, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      9, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      9, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      9, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      9, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     10, Layer:          802.11, pkts from network: 0
Node:     10, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     10, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     10, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     10, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     10, Layer:          802.11, retx pkts due to CTS timeout: 410
Node:     10, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     10, Layer:          802.11, pkt drops due to retx limit: 0
Node:     10, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     10, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     10, Layer:    AppCbrClient, (0) Server address: 7
Node:     10, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     10, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     10, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     10, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     10, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     10, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     11, Layer:          802.11, pkts from network: 0
Node:     11, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     11, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     11, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     11, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     11, Layer:          802.11, retx pkts due to CTS timeout: 383
Node:     11, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     11, Layer:          802.11, pkt drops due to retx limit: 0
Node:     11, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     11, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     11, Layer:    AppCbrClient, (0) Server address: 2
Node:     11, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     11, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     11, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     11, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     11, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     11, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     12, Layer:          802.11, pkts from network: 0
Node:     12, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     12, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     12, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     12, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     12, Layer:          802.11, retx pkts due to CTS timeout: 438
Node:     12, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     12, Layer:          802.11, pkt drops due to retx limit: 0
Node:     12, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     12, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     12, Layer:    AppCbrClient, (0) Server address: 6
Node:     12, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     12, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     12, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     12, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     12, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     12, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     13, Layer:          802.11, pkts from network: 0
Node:     13, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:     13, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     13, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:     13, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     13, Layer:          802.11, retx pkts due to CTS timeout: 420
Node:     13, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     13, Layer:          802.11, pkt drops due to retx limit: 0
Node:     13, Layer:          802.11, RTS Packets ignored due to Busy Channel 62
Node:     13, Layer:          802.11, RTS Packets ignored due to NAV 2
Node:     13, Layer:    AppCbrClient, (0) Server address: 5
Node:     13, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     13, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     13, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     13, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     13, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     13, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     14, Layer:          802.11, pkts from network: 0
Node:     14, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     14, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     14, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     14, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     14, Layer:          802.11, retx pkts due to CTS timeout: 390
Node:     14, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     14, Layer:          802.11, pkt drops due to retx limit: 0
Node:     14, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     14, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     14, Layer:    AppCbrClient, (0) Server address: 2
Node:     14, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     14, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     14, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     14, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     14, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     14, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     15, Layer:          802.11, pkts from network: 0
Node:     15, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     15, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     15, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     15, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     15, Layer:          802.11, retx pkts due to CTS timeout: 424
Node:     15, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     15, Layer:          802.11, pkt drops due to retx limit: 0
Node:     15, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     15, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     15, Layer:    AppCbrClient, (0) Server address: 3
Node:     15, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     15, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     15, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     15, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     15, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     15, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000