Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 638
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 632
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 434
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 6
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 2
Node:      0, Layer:    AppCbrServer, (0) Client address: 8
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.232595499
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.150500192
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.171281516
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      0, Layer:    AppCbrClient, (1) Server address: 8
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150160163823, end = 150538035497 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 167421 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 632
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 338
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 428
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150176194725, end = 150541664197 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 173103 bps
Node:      1, Layer:    AppCbrClient, (0) Server address: 7
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 922
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 1221
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 443
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrServer, (0) Client address: 11
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.255353865
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.260833919
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.226417495
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      2, Layer:    AppCbrServer, (0) Client address: 14
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.202373676
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.231471823
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.163606385
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      2, Layer:    AppCbrClient, (1) Server address: 6
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150250294536, end = 160250294536 ns (closed), bytes sent = 10 B, bytes recv = 76 B, throughput = 8 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1221
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 1222
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 481
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 59
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 5
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150251606836, end = 160278442295 ns (closed), bytes sent = 76 B, bytes recv =  10 B, throughput = 7 bps
Node:      3, Layer:    AppCbrServer, (0) Client address: 15
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.285234947
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.127133438
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.173334113
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      3, Layer:    AppCbrClient, (0) Server address: 15
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      4, Layer:          802.11, pkts from network: 0
Node:      4, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      4, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      4, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      4, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, retx pkts due to CTS timeout: 430
Node:      4, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      4, Layer:          802.11, pkt drops due to retx limit: 0
Node:      4, Layer:          802.11, RTS Packets ignored due to Busy Channel 69
Node:      4, Layer:          802.11, RTS Packets ignored due to NAV 3
Node:      4, Layer:    AppCbrClient, (0) Server address: 12
Node:      4, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      4, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      4, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      4, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      4, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      4, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      5, Layer:          802.11, pkts from network: 0
Node:      5, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:      5, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      5, Layer:          802.11, UCAST pkts rcvd clearly: 900
Node:      5, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      5, Layer:          802.11, retx pkts due to CTS timeout: 480
Node:      5, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      5, Layer:          802.11, pkt drops due to retx limit: 0
Node:      5, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      5, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      5, Layer:    AppCbrServer, (0) Client address: 13
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.164482338
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.081650030
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.192743970
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      5, Layer:    AppCbrClient, (0) Server address: 13
Node:      5, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      5, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      5, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      5, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      5, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      5, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      6, Layer:          802.11, pkts from network: 0
Node:      6, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1500
Node:      6, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      6, Layer:          802.11, UCAST pkts rcvd clearly: 1800
Node:      6, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, retx pkts due to CTS timeout: 524
Node:      6, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      6, Layer:          802.11, pkt drops due to retx limit: 0
Node:      6, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      6, Layer:          802.11, RTS Packets ignored due to NAV 5
Node:      6, Layer:    AppCbrServer, (1) Client address: 2
Node:      6, Layer:    AppCbrServer, (1) First packet received at [s]: 0.186755065
Node:      6, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.209232789
Node:      6, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.171552491
Node:      6, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (1) Throughput (bits per second): 6001
Node:      6, Layer:    AppCbrServer, (0) Client address: 12
Node:      6, Layer:    AppCbrServer, (0) First packet received at [s]: 0.179139861
Node:      6, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.066971659
Node:      6, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.170256447
Node:      6, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      6, Layer:    AppCbrClient, (0) Server address: 12
Node:      6, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      6, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      6, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      6, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      6, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      6, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      7, Layer:          802.11, pkts from network: 0
Node:      7, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:      7, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      7, Layer:          802.11, UCAST pkts rcvd clearly: 1200
Node:      7, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      7, Layer:          802.11, retx pkts due to CTS timeout: 457
Node:      7, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      7, Layer:          802.11, pkt drops due to retx limit: 0
Node:      7, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      7, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      7, Layer:    AppCbrServer, (0) Client address: 10
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.270042070
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.282998484
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.218797831
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      7, Layer:    AppCbrServer, (0) Client address: 1
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.141819461
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.157799398
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.163921541
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      7, Layer:    AppCbrClient, (0) Server address: 11
Node:      7, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      7, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      7, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      7, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      7, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      7, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      8, Layer:          802.11, pkts from network: 0
Node:      8, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:      8, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      8, Layer:          802.11, UCAST pkts rcvd clearly: 1200
Node:      8, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, retx pkts due to CTS timeout: 470
Node:      8, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      8, Layer:          802.11, pkt drops due to retx limit: 0
Node:      8, Layer:          802.11, RTS Packets ignored due to Busy Channel 79
Node:      8, Layer:          802.11, RTS Packets ignored due to NAV 6
Node:      8, Layer:    AppCbrServer, (0) Client address: 9
Node:      8, Layer:    AppCbrServer, (0) First packet received at [s]: 0.277441127
Node:      8, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.246061939
Node:      8, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.266166237
Node:      8, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      8, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      8, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      8, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:      8, Layer:    AppCbrServer, (1) Client address: 0
Node:      8, Layer:    AppCbrServer, (1) First packet received at [s]: 0.240539899
Node:      8, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.216590101
Node:      8, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.171361119
Node:      8, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      8, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      8, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      8, Layer:    AppCbrServer, (1) Throughput (bits per second): 6002
Node:      8, Layer:    AppCbrClient, (0) Server address: 0
Node:      8, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      8, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      8, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      8, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      8, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      8, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      9, Layer:          802.11, pkts from network: 0
Node:      9, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      9, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      9, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      9, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      9, Layer:          802.11, retx pkts due to CTS timeout: 529
Node:      9, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      9, Layer:          802.11, pkt drops due to retx limit: 0
Node:      9, Layer:          802.11, RTS Packets ignored due to Busy Channel 6
Node:      9, Layer:          802.11, RTS Packets ignored due to NAV 3
Node:      9, Layer:    AppCbrClient, (0) Server address: 8
Node:      9, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      9, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      9, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      9, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      9, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      9, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     10, Layer:          802.11, pkts from network: 0
Node:     10, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:     10, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     10, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:     10, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     10, Layer:          802.11, retx pkts due to CTS timeout: 431
Node:     10, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     10, Layer:          802.11, pkt drops due to retx limit: 0
Node:     10, Layer:          802.11, RTS Packets ignored due to Busy Channel 17
Node:     10, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     10, Layer:    AppCbrClient, (0) Server address: 7
Node:     10, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     10, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     10, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     10, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     10, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     10, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     11, Layer:          802.11, pkts from network: 0
Node:     11, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 900
Node:     11, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     11, Layer:          802.11, UCAST pkts rcvd clearly: 900
Node:     11, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     11, Layer:          802.11, retx pkts due to CTS timeout: 455
Node:     11, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     11, Layer:          802.11, pkt drops due to retx limit: 0
Node:     11, Layer:          802.11, RTS Packets ignored due to Busy Channel 5
Node:     11, Layer:          802.11, RTS Packets ignored due to NAV 8
Node:     11, Layer:    AppCbrServer, (0) Client address: 7
Node:     11, Layer:    AppCbrServer, (0) First packet received at [s]: 0.171786738
Node:     11, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.187176342
Node:     11, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.187082336
Node:     11, Layer:    AppCbrServer, (0) Session status: Not closed
Node:     11, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:     11, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:     11, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:     11, Layer:    AppCbrClient, (0) Server address: 2
Node:     11, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     11, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     11, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     11, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     11, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     11, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     12, Layer:          802.11, pkts from network: 0
Node:     12, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     12, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     12, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:     12, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     12, Layer:          802.11, retx pkts due to CTS timeout: 442
Node:     12, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     12, Layer:          802.11, pkt drops due to retx limit: 0
Node:     12, Layer:          802.11, RTS Packets ignored due to Busy Channel 4
Node:     12, Layer:          802.11, RTS Packets ignored due to NAV 10
Node:     12, Layer:    AppCbrServer, (0) Client address: 4
Node:     12, Layer:    AppCbrServer, (0) First packet received at [s]: 0.217046091
Node:     12, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.290337954
Node:     12, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.246483070
Node:     12, Layer:    AppCbrServer, (0) Session status: Not closed
Node:     12, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:     12, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:     12, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:     12, Layer:    AppCbrServer, (0) Client address: 6
Node:     12, Layer:    AppCbrServer, (0) First packet received at [s]: 0.194943049
Node:     12, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.103588155
Node:     12, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.163897406
Node:     12, Layer:    AppCbrServer, (0) Session status: Not closed
Node:     12, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:     12, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:     12, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:     12, Layer:    AppCbrClient, (0) Server address: 6
Node:     12, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     12, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     12, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     12, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     12, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     12, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     13, Layer:          802.11, pkts from network: 0
Node:     13, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:     13, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     13, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:     13, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     13, Layer:          802.11, retx pkts due to CTS timeout: 445
Node:     13, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     13, Layer:          802.11, pkt drops due to retx limit: 0
Node:     13, Layer:          802.11, RTS Packets ignored due to Busy Channel 72
Node:     13, Layer:          802.11, RTS Packets ignored due to NAV 4
Node:     13, Layer:    AppCbrServer, (0) Client address: 5
Node:     13, Layer:    AppCbrServer, (0) First packet received at [s]: 0.127236725
Node:     13, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.223857821
Node:     13, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.191650741
Node:     13, Layer:    AppCbrServer, (0) Session status: Not closed
Node:     13, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:     13, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:     13, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:     13, Layer:    AppCbrClient, (0) Server address: 5
Node:     13, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     13, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     13, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     13, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     13, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     13, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     14, Layer:          802.11, pkts from network: 0
Node:     14, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     14, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     14, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:     14, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     14, Layer:          802.11, retx pkts due to CTS timeout: 381
Node:     14, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     14, Layer:          802.11, pkt drops due to retx limit: 0
Node:     14, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:     14, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:     14, Layer:    AppCbrClient, (0) Server address: 2
Node:     14, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     14, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     14, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     14, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     14, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     14, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:     15, Layer:          802.11, pkts from network: 0
Node:     15, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:     15, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:     15, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:     15, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:     15, Layer:          802.11, retx pkts due to CTS timeout: 455
Node:     15, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:     15, Layer:          802.11, pkt drops due to retx limit: 0
Node:     15, Layer:          802.11, RTS Packets ignored due to Busy Channel 2
Node:     15, Layer:          802.11, RTS Packets ignored due to NAV 15
Node:     15, Layer:    AppCbrServer, (0) Client address: 3
Node:     15, Layer:    AppCbrServer, (0) First packet received at [s]: 0.292699347
Node:     15, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.172458421
Node:     15, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.168941387
Node:     15, Layer:    AppCbrServer, (0) Session status: Not closed
Node:     15, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:     15, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:     15, Layer:    AppCbrServer, (0) Throughput (bits per second): 6002
Node:     15, Layer:    AppCbrClient, (0) Server address: 3
Node:     15, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:     15, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:     15, Layer:    AppCbrClient, (0) Session status: Not closed
Node:     15, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:     15, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:     15, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000