Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 338
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 33
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 315
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      0, Layer:    AppCbrClient, (1) Server address: 3
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150034886286, end = 150343223276 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 205178 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 333
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 338
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 310
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150039249188, end = 150346671976 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 205788 bps
Node:      1, Layer:    AppCbrServer, (1) Client address: 2
Node:      1, Layer:    AppCbrServer, (1) First packet received at [s]: 0.023126760
Node:      1, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.022746760
Node:      1, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.018520170
Node:      1, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      1, Layer:    AppCbrClient, (0) Server address: 2
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 322
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 622
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 312
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrServer, (0) Client address: 1
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.030426102
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.007608300
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.018743046
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrServer, (0) Client address: 3
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.007988300
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.030126102
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.019592682
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrClient, (1) Server address: 1
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150036229180, end = 160036229180 ns (closed), bytes sent = 9 B, bytes recv = 851 B, throughput = 7 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 322
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 322
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 310
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150037561480, end = 160037289480 ns (closed), bytes sent = 851 B, bytes recv =  9 B, throughput = 7 bps
Node:      3, Layer:    AppCbrServer, (1) Client address: 0
Node:      3, Layer:    AppCbrServer, (1) First packet received at [s]: 0.015527642
Node:      3, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.015007642
Node:      3, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.019933607
Node:      3, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      3, Layer:    AppCbrClient, (0) Server address: 2
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000