Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 638
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 332
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 324
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      0, Layer:    AppCbrClient, (1) Server address: 1
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150043570462, end = 150343445327 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 210967 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 332
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 338
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 327
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150047793364, end = 150346694027 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 211655 bps
Node:      1, Layer:    AppCbrServer, (1) Client address: 0
Node:      1, Layer:    AppCbrServer, (1) First packet received at [s]: 0.015527642
Node:      1, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.030586102
Node:      1, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.020294462
Node:      1, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      1, Layer:    AppCbrClient, (0) Server address: 3
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 323
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 323
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 318
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrServer, (0) Client address: 3
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.007988300
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.015607560
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.019740308
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrClient, (1) Server address: 3
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150045108664, end = 160045108664 ns (closed), bytes sent = 10 B, bytes recv = 528 B, throughput = 8 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 323
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 623
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 321
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150046440964, end = 160046168964 ns (closed), bytes sent = 528 B, bytes recv =  10 B, throughput = 8 bps
Node:      3, Layer:    AppCbrServer, (0) Client address: 1
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.037930402
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.038450502
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.035733594
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      3, Layer:    AppCbrServer, (1) Client address: 2
Node:      3, Layer:    AppCbrServer, (1) First packet received at [s]: 0.023126760
Node:      3, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.023246842
Node:      3, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.019559750
Node:      3, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      3, Layer:    AppCbrClient, (0) Server address: 2
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000