Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 338
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 332
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 341
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      0, Layer:    AppCbrServer, (0) Client address: 8
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.125466895
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.110663187
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.094324201
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      0, Layer:    AppCbrClient, (1) Server address: 8
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150087826335, end = 150330646727 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 260538 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 632
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 638
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 363
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150104157219, end = 150333615427 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 275710 bps
Node:      1, Layer:    AppCbrServer, (0) Client address: 7
Node:      1, Layer:    AppCbrServer, (0) First packet received at [s]: 0.132976166
Node:      1, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.103368682
Node:      1, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.099649500
Node:      1, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      1, Layer:    AppCbrClient, (0) Server address: 7
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1510
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 1809
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 410
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrServer, (0) Client address: 4
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.103404111
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.029931184
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.088630166
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      2, Layer:    AppCbrServer, (0) Client address: 6
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.096004662
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.066527523
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.092103645
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrClient, (1) Server address: 6
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150155426637, end = 160155426637 ns (closed), bytes sent = 3 B, bytes recv = 2 B, throughput = 2 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 909
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 910
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 402
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150158526197, end = 160156486937 ns (closed), bytes sent = 2 B, bytes recv =  3 B, throughput = 2 bps
Node:      3, Layer:    AppCbrServer, (0) Client address: 5
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.110728024
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.118272424
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.104467512
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      3, Layer:    AppCbrClient, (0) Server address: 5
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      4, Layer:          802.11, pkts from network: 0
Node:      4, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      4, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      4, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, retx pkts due to CTS timeout: 352
Node:      4, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      4, Layer:          802.11, pkt drops due to retx limit: 0
Node:      4, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      4, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      4, Layer:    AppCbrClient, (0) Server address: 2
Node:      4, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      4, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      4, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      4, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      4, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      4, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      5, Layer:          802.11, pkts from network: 0
Node:      5, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      5, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      5, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:      5, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      5, Layer:          802.11, retx pkts due to CTS timeout: 401
Node:      5, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      5, Layer:          802.11, pkt drops due to retx limit: 0
Node:      5, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      5, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      5, Layer:    AppCbrServer, (0) Client address: 3
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.081406024
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.132936166
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.099146740
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      5, Layer:    AppCbrClient, (0) Server address: 3
Node:      5, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      5, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      5, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      5, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      5, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      5, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      6, Layer:          802.11, pkts from network: 0
Node:      6, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      6, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      6, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      6, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, retx pkts due to CTS timeout: 363
Node:      6, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      6, Layer:          802.11, pkt drops due to retx limit: 0
Node:      6, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      6, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      6, Layer:    AppCbrServer, (1) Client address: 2
Node:      6, Layer:    AppCbrServer, (1) First packet received at [s]: 0.066827300
Node:      6, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.073866901
Node:      6, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.091745330
Node:      6, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      6, Layer:    AppCbrClient, (0) Server address: 2
Node:      6, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      6, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      6, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      6, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      6, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      6, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      7, Layer:          802.11, pkts from network: 0
Node:      7, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      7, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      7, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:      7, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      7, Layer:          802.11, retx pkts due to CTS timeout: 383
Node:      7, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      7, Layer:          802.11, pkt drops due to retx limit: 0
Node:      7, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      7, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      7, Layer:    AppCbrServer, (0) Client address: 1
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.118112424
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.096024282
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.098947047
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      7, Layer:    AppCbrClient, (0) Server address: 1
Node:      7, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      7, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      7, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      7, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      7, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      7, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      8, Layer:          802.11, pkts from network: 0
Node:      8, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      8, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      8, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      8, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, retx pkts due to CTS timeout: 348
Node:      8, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      8, Layer:          802.11, pkt drops due to retx limit: 0
Node:      8, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      8, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      8, Layer:    AppCbrServer, (1) Client address: 0
Node:      8, Layer:    AppCbrServer, (1) First packet received at [s]: 0.074106772
Node:      8, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.125606787
Node:      8, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.094508964
Node:      8, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      8, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      8, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      8, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      8, Layer:    AppCbrClient, (0) Server address: 0
Node:      8, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      8, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      8, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      8, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      8, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      8, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000