Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 338
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 332
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 352
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      0, Layer:    AppCbrServer, (0) Client address: 8
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.088765292
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.059288180
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.078760153
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      0, Layer:    AppCbrClient, (1) Server address: 1
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150065367539, end = 150350203924 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 222106 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 332
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 638
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 344
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150067099839, end = 150353632624 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 220791 bps
Node:      1, Layer:    AppCbrServer, (0) Client address: 7
Node:      1, Layer:    AppCbrServer, (0) First packet received at [s]: 0.110853224
Node:      1, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.103354160
Node:      1, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.082979287
Node:      1, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      1, Layer:    AppCbrServer, (1) Client address: 0
Node:      1, Layer:    AppCbrServer, (1) First packet received at [s]: 0.030046209
Node:      1, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.007848300
Node:      1, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.044711576
Node:      1, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      1, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      1, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      1, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      1, Layer:    AppCbrClient, (0) Server address: 2
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 1232
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 1531
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 398
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrServer, (0) Client address: 6
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.081486142
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.110723661
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.079599513
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrServer, (0) Client address: 1
Node:      2, Layer:    AppCbrServer, (0) First packet received at [s]: 0.059463199
Node:      2, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.015127500
Node:      2, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.045242407
Node:      2, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      2, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      2, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      2, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      2, Layer:    AppCbrClient, (1) Server address: 3
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150116765423, end = 160116765423 ns (closed), bytes sent = 14 B, bytes recv = 220 B, throughput = 11 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 631
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 932
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 377
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150127066283, end = 160117825723 ns (closed), bytes sent = 220 B, bytes recv =  14 B, throughput = 11 bps
Node:      3, Layer:    AppCbrServer, (0) Client address: 5
Node:      3, Layer:    AppCbrServer, (0) First packet received at [s]: 0.103468824
Node:      3, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.073906758
Node:      3, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.086134895
Node:      3, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      3, Layer:    AppCbrServer, (1) Client address: 2
Node:      3, Layer:    AppCbrServer, (1) First packet received at [s]: 0.052163740
Node:      3, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.022426760
Node:      3, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.040967534
Node:      3, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      3, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      3, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      3, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      3, Layer:    AppCbrClient, (0) Server address: 4
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      4, Layer:          802.11, pkts from network: 0
Node:      4, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      4, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      4, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      4, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, retx pkts due to CTS timeout: 349
Node:      4, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      4, Layer:          802.11, pkt drops due to retx limit: 0
Node:      4, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      4, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      4, Layer:    AppCbrServer, (0) Client address: 3
Node:      4, Layer:    AppCbrServer, (0) First packet received at [s]: 0.096069485
Node:      4, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.095974800
Node:      4, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.101178349
Node:      4, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      4, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      4, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      4, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      4, Layer:    AppCbrClient, (0) Server address: 5
Node:      4, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      4, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      4, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      4, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      4, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      4, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      5, Layer:          802.11, pkts from network: 0
Node:      5, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      5, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      5, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:      5, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      5, Layer:          802.11, retx pkts due to CTS timeout: 367
Node:      5, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      5, Layer:          802.11, pkt drops due to retx limit: 0
Node:      5, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      5, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      5, Layer:    AppCbrServer, (0) Client address: 4
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.007688300
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.044604811
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.043782212
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      5, Layer:    AppCbrClient, (0) Server address: 3
Node:      5, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      5, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      5, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      5, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      5, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      5, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      6, Layer:          802.11, pkts from network: 0
Node:      6, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      6, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      6, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, retx pkts due to CTS timeout: 353
Node:      6, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      6, Layer:          802.11, pkt drops due to retx limit: 0
Node:      6, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      6, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      6, Layer:    AppCbrClient, (0) Server address: 2
Node:      6, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      6, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      6, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      6, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      6, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      6, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      7, Layer:          802.11, pkts from network: 0
Node:      7, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      7, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      7, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      7, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      7, Layer:          802.11, retx pkts due to CTS timeout: 375
Node:      7, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      7, Layer:          802.11, pkt drops due to retx limit: 0
Node:      7, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      7, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      7, Layer:    AppCbrClient, (0) Server address: 1
Node:      7, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      7, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      7, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      7, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      7, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      7, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      8, Layer:          802.11, pkts from network: 0
Node:      8, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      8, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      8, Layer:          802.11, UCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, retx pkts due to CTS timeout: 351
Node:      8, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      8, Layer:          802.11, pkt drops due to retx limit: 0
Node:      8, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      8, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      8, Layer:    AppCbrClient, (0) Server address: 0
Node:      8, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      8, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      8, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      8, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      8, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      8, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000