Node:      0, Layer:          802.11, pkts from network: 0
Node:      0, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 338
Node:      0, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      0, Layer:          802.11, UCAST pkts rcvd clearly: 632
Node:      0, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      0, Layer:          802.11, retx pkts due to CTS timeout: 347
Node:      0, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      0, Layer:          802.11, pkt drops due to retx limit: 0
Node:      0, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      0, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      0, Layer:    AppCbrServer, (0) Client address: 7
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.113032665
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.111708569
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.112548237
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      0, Layer:    AppCbrServer, (0) Client address: 8
Node:      0, Layer:    AppCbrServer, (0) First packet received at [s]: 0.105508265
Node:      0, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.104244169
Node:      0, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.083845317
Node:      0, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      0, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      0, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      0, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      0, Layer:    AppCbrClient, (1) Server address: 7
Node:      0, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      0, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      0, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      0, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      0, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      0, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      0, Layer:    AppFtpClient, from 0 to 1 (cid = 1), start = 150092197367, end = 150339568950 ns (closed), bytes sent = 7908 B, bytes recv = 279 B, throughput = 255744 bps
Node:      1, Layer:          802.11, pkts from network: 0
Node:      1, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 632
Node:      1, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      1, Layer:          802.11, UCAST pkts rcvd clearly: 338
Node:      1, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      1, Layer:          802.11, retx pkts due to CTS timeout: 370
Node:      1, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      1, Layer:          802.11, pkt drops due to retx limit: 0
Node:      1, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      1, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      1, Layer:    AppFtpServer, from 0 to 1 (cid = 2), start = 150111214669, end = 150342577650 ns (closed) bytes sent = 279 B, bytes recv = 7908 B, throughput = 273440 bps
Node:      1, Layer:    AppCbrClient, (0) Server address: 6
Node:      1, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      1, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      1, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      1, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      1, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      1, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      2, Layer:          802.11, pkts from network: 0
Node:      2, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 932
Node:      2, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      2, Layer:          802.11, UCAST pkts rcvd clearly: 631
Node:      2, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      2, Layer:          802.11, retx pkts due to CTS timeout: 395
Node:      2, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      2, Layer:          802.11, pkt drops due to retx limit: 0
Node:      2, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      2, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      2, Layer:    AppCbrClient, (1) Server address: 5
Node:      2, Layer:    AppCbrClient, (1) First packet sent at [s]: 0.000000000
Node:      2, Layer:    AppCbrClient, (1) Last packet sent at [s]: 598.000000000
Node:      2, Layer:    AppCbrClient, (1) Session status: Not closed
Node:      2, Layer:    AppCbrClient, (1) Total number of bytes sent: 450000
Node:      2, Layer:    AppCbrClient, (1) Total number of packets sent: 300
Node:      2, Layer:    AppCbrClient, (1) Throughput (bits per second): 6000
Node:      2, Layer: AppTelnetClient, from 2 to 3 (cid = 1), start = 150109747635, end = 160109747635 ns (closed), bytes sent = 14 B, bytes recv = 114 B, throughput = 11 bps
Node:      3, Layer:          802.11, pkts from network: 0
Node:      3, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 931
Node:      3, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      3, Layer:          802.11, UCAST pkts rcvd clearly: 632
Node:      3, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      3, Layer:          802.11, retx pkts due to CTS timeout: 382
Node:      3, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      3, Layer:          802.11, pkt drops due to retx limit: 0
Node:      3, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      3, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      3, Layer: AppTelnetServer, from 2 to 3 (cid = 2), start = 150122701715, end = 160114294531 ns (closed), bytes sent = 114 B, bytes recv =  14 B, throughput = 11 bps
Node:      3, Layer:    AppCbrClient, (0) Server address: 5
Node:      3, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      3, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      3, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      3, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      3, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      3, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      4, Layer:          802.11, pkts from network: 0
Node:      4, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      4, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      4, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      4, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      4, Layer:          802.11, retx pkts due to CTS timeout: 374
Node:      4, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      4, Layer:          802.11, pkt drops due to retx limit: 0
Node:      4, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      4, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      4, Layer:    AppCbrClient, (0) Server address: 5
Node:      4, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      4, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      4, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      4, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      4, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      4, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      5, Layer:          802.11, pkts from network: 0
Node:      5, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      5, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      5, Layer:          802.11, UCAST pkts rcvd clearly: 1200
Node:      5, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      5, Layer:          802.11, retx pkts due to CTS timeout: 352
Node:      5, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      5, Layer:          802.11, pkt drops due to retx limit: 0
Node:      5, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      5, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      5, Layer:    AppCbrServer, (0) Client address: 3
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.121482712
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.119902753
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.085607943
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6001
Node:      5, Layer:    AppCbrServer, (1) Client address: 2
Node:      5, Layer:    AppCbrServer, (1) First packet received at [s]: 0.052163882
Node:      5, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.059463448
Node:      5, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.044859904
Node:      5, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (1) Throughput (bits per second): 6000
Node:      5, Layer:    AppCbrServer, (0) Client address: 4
Node:      5, Layer:    AppCbrServer, (0) First packet received at [s]: 0.007688300
Node:      5, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.037285586
Node:      5, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.043769787
Node:      5, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      5, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      5, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      5, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      5, Layer:    AppCbrClient, (0) Server address: 6
Node:      5, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      5, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      5, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      5, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      5, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      5, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      6, Layer:          802.11, pkts from network: 0
Node:      6, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      6, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      6, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:      6, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      6, Layer:          802.11, retx pkts due to CTS timeout: 337
Node:      6, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      6, Layer:          802.11, pkt drops due to retx limit: 0
Node:      6, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      6, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      6, Layer:    AppCbrServer, (0) Client address: 1
Node:      6, Layer:    AppCbrServer, (0) First packet received at [s]: 0.097598045
Node:      6, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.052114286
Node:      6, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.104122685
Node:      6, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      6, Layer:    AppCbrServer, (0) Client address: 5
Node:      6, Layer:    AppCbrServer, (0) First packet received at [s]: 0.044784538
Node:      6, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.015227684
Node:      6, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.044953406
Node:      6, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      6, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      6, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      6, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      6, Layer:    AppCbrClient, (0) Server address: 7
Node:      6, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      6, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      6, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      6, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      6, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      6, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      7, Layer:          802.11, pkts from network: 0
Node:      7, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 300
Node:      7, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      7, Layer:          802.11, UCAST pkts rcvd clearly: 600
Node:      7, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      7, Layer:          802.11, retx pkts due to CTS timeout: 356
Node:      7, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      7, Layer:          802.11, pkt drops due to retx limit: 0
Node:      7, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      7, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      7, Layer:    AppCbrServer, (1) Client address: 0
Node:      7, Layer:    AppCbrServer, (1) First packet received at [s]: 0.129087112
Node:      7, Layer:    AppCbrServer, (1) Last packet received at [s]: 598.127167153
Node:      7, Layer:    AppCbrServer, (1) Average end-to-end delay [s]: 0.108565382
Node:      7, Layer:    AppCbrServer, (1) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (1) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (1) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (1) Throughput (bits per second): 6001
Node:      7, Layer:    AppCbrServer, (0) Client address: 6
Node:      7, Layer:    AppCbrServer, (0) First packet received at [s]: 0.022546719
Node:      7, Layer:    AppCbrServer, (0) Last packet received at [s]: 598.022506901
Node:      7, Layer:    AppCbrServer, (0) Average end-to-end delay [s]: 0.044564705
Node:      7, Layer:    AppCbrServer, (0) Session status: Not closed
Node:      7, Layer:    AppCbrServer, (0) Total number of bytes received: 450000
Node:      7, Layer:    AppCbrServer, (0) Total number of packets received: 300
Node:      7, Layer:    AppCbrServer, (0) Throughput (bits per second): 6000
Node:      7, Layer:    AppCbrClient, (0) Server address: 0
Node:      7, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      7, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      7, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      7, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      7, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      7, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000
Node:      8, Layer:          802.11, pkts from network: 0
Node:      8, Layer:          802.11, UCAST (non-frag) pkts sent to chanl: 600
Node:      8, Layer:          802.11, BCAST pkts sent to chanl: 0
Node:      8, Layer:          802.11, UCAST pkts rcvd clearly: 300
Node:      8, Layer:          802.11, BCAST pkts rcvd clearly: 0
Node:      8, Layer:          802.11, retx pkts due to CTS timeout: 378
Node:      8, Layer:          802.11, retx pkts due to ACK timeout: 0
Node:      8, Layer:          802.11, pkt drops due to retx limit: 0
Node:      8, Layer:          802.11, RTS Packets ignored due to Busy Channel 0
Node:      8, Layer:          802.11, RTS Packets ignored due to NAV 0
Node:      8, Layer:    AppCbrClient, (0) Server address: 0
Node:      8, Layer:    AppCbrClient, (0) First packet sent at [s]: 0.000000000
Node:      8, Layer:    AppCbrClient, (0) Last packet sent at [s]: 598.000000000
Node:      8, Layer:    AppCbrClient, (0) Session status: Not closed
Node:      8, Layer:    AppCbrClient, (0) Total number of bytes sent: 450000
Node:      8, Layer:    AppCbrClient, (0) Total number of packets sent: 300
Node:      8, Layer:    AppCbrClient, (0) Throughput (bits per second): 6000